**მოწვევა ბაზრის კვლევაში მონაწილეობის მიღების თაობაზე**

**საქართველოს ოკუპირებული ტერიტორიებიდან დევნილთა, შრომის, ჯანმრთელობისა და სოციალური დაცვის სამინისტრო**

**აცხადებს ბაზრის კვლევას**

**ფოტო აპარატურის შესყიდვის მიზნით**

საქართველოს ოკუპირებული ტერიტორიებიდან დევნილთა, შრომის, ჯანმრთელობისა და სოციალური დაცვის სამინისტრო, COVID-19-ის წინააღმდეგ სწრაფი რეაგირების პროექტის ფარგლებში, მსოფლიო ბანკის შესყიდვების წესებისა და პირობების შესაბამისად გეგმავს ფოტოაპარატურის შესყიდვას:

გთხოვთ, შესასყიდი საქონლის სპეციფიკაციები და ბაზრის კვლევაში მონაწილეობის მისაღებად მიმწოდებლისათვის განსაზღვრული მოთხოვნები იხილოთ თანდართულ დოკუმენტში და წარმოადგინოთ წინადადება მითითებული ფასების ცხრილის ფორმატის შესაბამისად.

წინადადებების წარმოდგენის ბოლო ვადაა 2023 წლის 10 თებერვალი.

გთხოვთ, წინადადებები მოგვაწოდოთ შემდეგი ელექტრონული ფოსტის მისამართზე: ttoriashvili@moh.gov.ge და khamilakhvari@moh.gov.ge - სათაურით (subject line) ***წინადადება - ბაზრის კვლევა ფოტოაპარატურის შესყიდვის მიზნით***.

წინასწარ გიხდით მადლობას ბაზრის კვლევაში მონაწილეობის მიღებისთვის!

საკონტაქტო ინფორმაცია: საქართველოს ოკუპირებული ტერიტორიებიდან დევნილთა, შრომის, ჯანმრთელობისა და სოციალური დაცვის სამინისტრო

მსოფლიო ბანკის პროექტის განმახორციელებელი ჯგუფი:

თეა ტორიაშვილი - შესყიდვების კონულტანტი.

ტელ: 032 2 51 00 26 (შიდა - 05 06)

**Invitation to participate in Market Research**

**The Ministry of Internally Displaced Persons from Occupied Territories, Labour, Health and Social Affairs of Georgia announces market research for procurement of Photographic Equipment**

The Ministry of Internally Displaced Persons from Occupied Territories, Labour, Health and Social Affairs of Georgia intends to procure Photographic Equipment in compliance with the World Bank Procurement Rules and Regulations within the framework of the **Emergency COVID-19 Response Project.**

Technical Specifications and other requirements to participate in market research are provided in attached document. Please, submit your offer in compliance with above referenced requirements and the price schedules provided in the attached document.

The deadline for submission of your offers in February 10, 2023.

The offers should be submitted to the following e-mail addresses: ttoriashvili@moh.gov.ge და khamilakhvari@moh.gov.ge - (subject line) Offer – ***market research for procurement of Photographic Equipment.***

Thank you in advance for participating in Market Research!

**Contact Information:** The Ministry of Internally Displaced Persons from Occupied Territories, Labour, Health and Social Affairs of Georgia

The World Bank Implementation Project:

Tea Toriashvili, Procurement Consultant.

Tel: 032 2 51 00 26 (Ext - 05 06)

**Technical Specifications/ტექნიკური სპეციფიკაციები**

|  |  |  |  |
| --- | --- | --- | --- |
| **Item No** | **Name of Goods / საქონლის დასახელება** | **Required Technical Specifications / მოთხოვნილის ტექნიკური სპეციფიკაციები** | **Technical Specifications to be filled by the Supplier / მომწოდებლის მიერ შესავსები ტექნიკური სპეციფიკაციები** |
| **1** | **Nikon Z9 Professional Camera**  | * Matrix - 45.7MP FX-Format Stacked CMOS Sensor
* Number of focus points of the hybrid system: 493
* Lens shutter: Z mount.
* Shooting speed: 1/32,000
* Continuous shooting speed: Raw - 20 frames/sec; JPEG - 30 frames/sec.
* Function of electronic shooter.
* XQD standard of memory cards.
* Sensor screen 3.2" diagonal 2.1mp color quality OLED screen.
* Viewfinder (EVF) „Dot Quad VGA EVF; frame coverage: 100%, magnification: 0,8x; color quality: 3.6 mp.
* Wi-Fi support.

**Warranty: Not less than 1 year**. |  |
| **2** | **Camera lens** | The camera set shall include 2 (two) types of camera lenses to be adjustable without converter:1. Nikon NIKKOR Z 24-120mm f/4 S Lens

Z-Mount Lens/FX Format1. Nikon NIKKOR Z DX 50-250mm f/4.5-6.3 VR Lens

Z-Mount Lens/DX Format**Warranty: Not less than 1 year** |  |
| **3** | **Rechargeable Lithium-ion spare battery for Nikon Z9** | Nikon EN-EL18d rechargeable Lithium-ion spare battery for Nikon Z9.Capacity: 3300 mAh, an output of 10.8V, and 36Wh. The battery can charge within the MH-33 charger and it can be used as a spare or replacement battery for the Nikon Z9. |  |
| **4** | **Camera metal cage** | Metal set of camera cage with top handle for Nikon Z9. Weight: not to exceed 300 g; dimensions: height including the handle: 229 mm, depth: 69.4 mm, width: 164 mm.**Warranty: not less than 1 year.**  |  |
| **5** | **Integrated wireless microphone system of the camera**  | Frequency range - A: 516 to 558 MHzThe set shall include: 1. Wireless microphone;
2. Microphone receiver;
3. Lavalier radio-microphone;
4. Microphone sponge

**Warranty: not less than 2 years** |  |
| **6** | **Rechargeable****batteries AA** | Multiple use, rechargeable AA batteries for microphone system. Each shall have at least 1.2V output capacity and at least 2550 mAh. **Warranty: not less than 1 year.** |  |
| **7** | **Battery charger** | Shall be adjustable to the above indicated AA batteries.**Warranty: not less than 1 year.** |  |
| **8** | **Camera backpack** | The backpack shall enable safe placing of the above-indicated camera, lenses, and accessories along with the laptop, which is required in the course of the field works execution. The backpack shall be made of such material that enables its applying under all weather conditions so as the gear not to get wet. |  |
| **9** | **64 GB memory card adjustable to Nikon Z9** | Read speed: not less than 440 MB/s. Record speed: not less than 400 MB/s.**Warranty: not less than 2 years.** |  |
| **10** | **Memory card reader adjustable to that memory card**  | Data transfer speed of at least up to 10 GB/s.**Warranty: not less than 1 year.** |  |
| **11** | **Tripod** | It shall be adjustable to the above-indicated camera. It shall be lightweight, and of Carbon Fiber material. The tripod shall be on 3 rubber feet. 75mm Half Ball/Flat Base Mount. Sliding PlateMeasures: 9.4" long with a sliding range of 3.7"Its weight shall not exceed 2 kg and payload is to be of at least 9 kg. It might be extended up to at least 154 cm. Plate ¨1/4"-20 and 3/8"-16 camera mounting screws. **Warranty: not less than 2 years.** |  |
| **12** | **Camera illumination** | Stepped variable color from 3200 to 5600K. Metal chassis construction.Integrated rechargeable battery Li-Ion. Dimming from 100 to 10% brightness. Snap-On diffusion filter should be Included. Two 1/4"-20 threaded mounting holes. Dimensions- no more than 7.4 x 5.8 x 2 inches. Weight not to exceed 250 grams.  |  |
| **13** | **Gimbal integrated stabilizer with its battery**  | It shall be of lightweight, made of carbon material, and at least of 1,5 kg weight so as to take the load of at least 4,5 kg.It shall have the built-in 1.8 -inch OLED full-color touchscreen. Battery life during operation shall be at least 12 hours. Charging time: not to exceed 2 hours. Temperature: from 5° to 40°C (41- 104°F), connections: (USB-C)Dimensions: folded - 268×276×68 mm (L×W×H, excluding camera, handle and extended grip/step); extended: 415×218×195 mm (L×W×H, height shall include grip and does not include extended grip/step); Gimbal shall be enclosed with the focus control system and all accessories:USB power cable (7.9")USB Type-C charging cable (15.7")USB Type-C multi-controlling cable (11.8")HDMI cable (7.9") out of mini HDMI Mini HDMI cable (7.9") out of mini HDMI Micro HDMI cable (7.9") out of mini HDMI **Warranty: not less than 6 months.** |  |
| **14** | **Lens**  | Lens to operate at far distance to be adjusted to Canon EOS 5d mark 4;Canon EF 70-200mm f/2.8L IS III USM**Warranty: not less than 1 year.** |  |
| **15** | **Filter for above-indicated lens**  | Chiaro Pro 77mm 99-UVBTS Brass UV **Warranty: not less than 1 year.** |  |
| **16** | **Filter** (for lens *Canon RF 24-70mm f/2.8 L IS USM***)** | Chiaro Pro 82mm 99-UVBTS Brass UV Filter**Warranty: not less than 1 year.** |  |
| **17** | **Camera flash to be adjusted to Canon EOS 5d mark 4;camera.**  | Canon Speedlite EL-1**Warranty: not less than 1 year.** |  |
| **18** | **Camera backpack** | The backpack shall enable safe placing of the above indicated camera, lens, and accessories along with the laptop, required in the course of the field works execution. The backpack shall me made of such material that enables its applying under all weather conditions so as the gear not to get wet.  |  |
| **19** | **External hard disc (for video/photo data storing)** | Capacity: no less than 5 TBInterface: USB 3.0Reverse compatibility with USB 2.0**Warranty: not less than 1 year.** |  |

**Note: The above mentioned equipment must be original not counterfeit. Should come in factory appropriate packaging and have appropriate documentation / ზემოხსენებული საქონელი უნდა იყოს ორიგინალი, ქარხნულ შეფუთვაში და თან ახლდეს შესაბამისი დოკუმენტაცია.**

|  |
| --- |
| **Price Schedule / ფასების ცხრილი** |
| 1 | 2 | 3 | 4 | 5 | 6 | 7 |
| **N°** | **Description of Goods / საქონლის აღწერა**  | **Country of Origin / წარმოშობის ქვეყანა** | **Delivery Date as defined by Incoterms / მოწოდების ვადა Incoterm-ის მიხედვით** | **Quantity and physical unit / რაოდენობა და განზომილების ერთეული** | **Unit price / ერთულის შირებულება** | **Total Price per (Col. 6+7) / ჯამური ღირებულება (სვეტი 6+)** |
| 1 | Nikon Z9 Professional Camera  |  |  | 2 pieces / ცალი |  |  |
| 2.1 | Camera lens - Nikon NIKKOR Z 24-120mm f/4 S Lens Z-Mount Lens/FX Format |  |  | 2 pieces / ცალი |  |  |
| 2.2 | Camera lens –Nikon NIKKOR Z DX 50-250mm f/4.5-6.3 VR Lens Z-Mount Lens/DX Format |  |  | 2 pieces /ცალი |  |  |
| 3 | Nikon EN-EL18d rechargeable Lithium-ion spare battery for Nikon Z9 |  |  | 2 pieces /ცალი |  |  |
| 4 | Camera metal cage |  |  | 2 pieces /ცალი |  |  |
| 5 | Integrated wireless microphone system of the camera  |  |  | 2 pieces /ცალი |  |  |
| 6 | Rechargeablebatteries AA  |  |  | 16 pieces / ცალი |  |  |
| 7 | Battery charger |  |  | 2 pieces / ცალი |  |  |
| 8 | Camera backpack |  |  | 2 pieces / ცალი |  |  |
| 9 | 64 GB memory card adjustable to Nikon Z9 |  |  | 4 pieces / ცალი |  |  |
| 10 | Memory card reader adjustable to that memory card  |  |  | 2 pieces / ცალი |  |  |
| 11 | Tripod |  |  | 2 pieces / ცალი |  |  |
| 12 | Camera illumination |  |  | 2 pieces / ცალი |  |  |
| 13 | Gimbal integrated stabilizer with its battery  |  |  | 1 piece / ცალი |  |  |
| 14 | Lens  |  |  | 1 piece / ცალი |  |  |
| 15 | Filter for above-indicated lens |  |  | 1 piece / ცალი |  |  |
| 16 | Filter (for lens Canon RF 24-70mm f/2.8 L IS USM) |  |  | 1 piece / ცალი |  |  |
| 17 | Camera flash to be adjusted to Canon EOS 5d mark 4 camera. |  |  | 1 piece / ცალი |  |  |
| 18 | Camera backpack |  |  | 1 piece / ცალი |  |  |
| 19 | External hard disc |  |  | 2 pieces / ცალი |  |  |
| **Total**  |  |

**Please, provide following information / გთხოვთ მიუთითოთ შემდეგი ინფორმაცია:**

* **General Experience:** The Supplier shall demonstrate that it has similar experience / **ზოგადი გამოცდილება:** მიმწოდებელმა უნდა აჩვენოს, რომ მას აქვს მსგავსი გამოცდილება
* **Specific Experience:** The Bidder shall demonstrate that it has successfully completed at least 1 contract of similar nature and complexity in the capacity of the Prime Contractor within the last 5 years. The Suppliers shall indicate contract values for successfully completed contracts / **სპეციალური გამოცდილება**: მიმწოდებელმა უნდა აჩვენოს, რომ მას, როგორც ძრითად კონტრაქტორს, აქვს წარმატებით განხორციელებული მსგავსი ხასიათის და სირთულის მინიმუმ ერთი კონტრაქტი ბოლო 5 წლის განმავლობაში. მიმწოდებელმა უნდა მიუთითოს წარმატებით შესრულებული კონტრაქტების ღირებულებები.
* **Expected delivery time and delivery term:** the Supplier shall indicate the time frame for the supply of the goods and delivery term as per Incoterms / **მოწოდების სავარაუდო ვადა და მოწოდების პირობა**: მიმწოდებელმა უნდა მიუთითოს საქონლის მოწოდების სავარაუდო ვადა და მოწოდების პირობა Incoterms-ის შესაბამისად.